Project:

Proposed specification prepared for



**Free-Standing Mono-Pitch Canopy**

1. Description: WeatherSpan Free-standing Mono-Pitch Aluminium Frame Canopy with Polycarbonate/Glass roof
2. Standard: To BS EN 1090
3. Manufacturer: Waverley Contract & Supply Ltd

 Rowan House, Guildford Road Trading Estate,

 Farnham, GU9 9PZ

 Tel. 01252 737973

 www.waverley.co.uk

 Contact: Michael Denyer

 Email. michael@waverley.co.uk

1. Type: Free-Standing Mono-Pitch
2. Dimensions: refer to schedule and drawings for size and locations
3. Frame:
	1. Aluminium extrusion, 6063 T6 grade
	2. 125mm rear legs with 125mm rear cross beam
	3. 110mm round/square legs with integral rainwater downpipe
	4. 130mm x 90mm heavy duty front profile with integral gutter with radiused/straight fascia.
	5. 60mm x 120mm roof beams
	6. Powdercoat finish to RAL….
4. Roof sheets: 16mm multiwall polycarbonate, weight 2.7kg/m2

7.1. Finish/ Colour: Clear 85% Light Transmission

 Or Opal 42% Light Transmission

Roof Sheets: 8.76mm laminate glass in clear finish, 20.8Kg/m2

1. Fixing: Galvanised steel base plate bolted to suitable concrete foundation
2. Rainwater management: FFL/connection underground
3. Accessories/ Other requirements:

 Post pads

 Side infill panels – polycarbonate or aluminium panels

 LED Lights

 Retractable Zip Screen roller blinds – motorised or manual

1. Manufacturers 10 Year Warranty on canopy system against manufacturing defects